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Product Specification
	Display Panel

	Panel 	
	10.1inches LED back-light/model:M101WXBI45-AA-01

	Active Area(mm)
	216.96 (W) ×135.60 (H) mm

	Aspect Ratio
	16:10

	Resolution
	1280×800

	Brightness
	280/350 cd/m2

	Contrast Ratio
	800:1

	Viewing Angle
	All angles ( R/L 89 (Min.), U/D 89 (Min.))

	Color 
	16.7Mcolors

	Color temperature
	5500K

	Backlight lamp life
	30000 hours

	Response time
	6ms

	System 

	Main board model
	SWH5128

	CPU
	Rockchip RK3126

	GPU 
	ARM Mali-400MP2 GPU

	Memory 
	DDR3 512Mbyte,

	Storage 
	8GB eMMC

	Operation system
	Android5.1

	Touch

	Model 
	/

	Touch type
	/

	Touch Points
	/

	Interpolation resolution
	/

	Touch accuracy
	/

	Response time
	/

	Enter mode
	/

	Smallest touch objects
	Single 
	/

	
	Multi-point
	/

	ports

	Signal port
	/

	Network ports
	LAN*1（10/100MEthernet），wifi (802.11n)、 blue-tooth(4.0)

	Storage extension
	 32GB（max）

	Other 
	USB(2.0)*1、RS232*1（3.5mm jack）、POE(24V)

	multimedia

	Media file formats
	video：MOV, MP4, AVI, MPG, 3PG

	
	audio：MP3

	
	picture：JPEG、BMP、PNG

	
	text：txt

	Play mode
	Landscape, vertical screen, full screen, and split screen

	Program transmission way
	USB, LAN, Wan transport

	Other parameters 

	Product Size(mm)
	239.9（H）×169.2（V）×26.8（D）

	Package Size(mm）
	333（H）×278（V）×75（D）

	VESA（mm）
	50*50

	Screen hanging mode
	Landscape, portrait

	[bookmark: OLE_LINK2]Menu language
	Chinese, English 

	Machine color
	Black

	Weight 
	net：0.5KG  gross：2.0KG

	Power Consumption
	12W(Max)

	Speaker
	stereo 1.5W x8Ω

	Watchdog timer
	/

	Timing function
	multiple time periods programmable power on/off

	Management software
	GTV

	Power supply
	DC 12V

	Working temperature
	0〜40℃

	Working humidity
	10% 〜 80%RH

	Storage environment
	- 10 ~ 50 ℃ temperature/ 10% ~ 90% RH humidity

	Accessories
	Warranty card * 1,Remote control * 1, certificate * 1, 12 v power adapter * 1,Network line* 1, safety and environmental considerations * 1,National standard power cord * 1,AAA battery * 2


	Certificates
	CCC
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Packaging
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